
Steps to apply the special settings:

  1) Connect to the scanner in PhoXi Control
  2) Trigger the scan
  3) Run "SetSettings.bat" and upon request please enter the parameter as number. 
     First put 1.25 as PatternScaleX and press enter, then put 1.25 as PatternScaleY and press enter.
     Write any key and press enter to close

  4) Trigger the scan to see if the change of settings has desired effect
  5) If the results are good and you want to keep this settings permanent, 
     check "SaveOnSet" checkbox and hit "Set" button or "Set and Store" depending of PhoXi Control version. 
	 The settings will be set as default settings that are used after
	 booting the device.
	 
If you want to restore the settings to original value, please enter 1 for both PatternScaleX and PatternScaleY


More information: support@photoneo.com